**Company Brief**

|  |  |  |
| --- | --- | --- |
| **Year Founded** | : | 2012 |
| **Location** | : | Batang, Central Java, Indonesia |
| **Factory Space** | : | Plot size: 68,000 m2  Built-up area: 28,200 m2 |
| **Industry** | : | Papermaking |
| **Products** | : | 100% recycled brown kraft paper (100-200 GSM) of the following types:   * Corrugating Medium * Test Liner |
| **Production Capacity** | : | 115,000 MT/year |
| **Markets Served** | : | * Domestic * International, including:   + China   + Southeast Asia   + South Asia   + Europe   + Middle East   + Africa   + ANZ   + Oceania |
| **Raw Material Source** | : | * Domestic * International, including:   + Southeast Asia   + Europe   + Australia   + Africa   + Middle East |
| **Main Machines** | : | * European paper machine * Machine width 4,500 mm * 2 headboxes with fourdrinier table * 51 dryers * German-made pond sizer (Bellmer) * Metso QCS and DCS * Valmet rewinder twin drum |
| **Boilers** | : | 3 Boilers:   * 1 x 20 tons * 2 x 10 tons |
| **Waste Water Treatment** | : | * 5,000 m3 per day * Designed to accommodate two paper machines |
| **Number of Employees** | : | 300 |
| **Electrical Power Supply** | : | PLN 8 Mva, backup generator 500 Kva |
| **Water Supply** | : | River and underground water source |
| **Additional Machines Procured but Not Installed** | : | * Disperger * Refiners |
| **Average Revenue Growth** | : | 9.6%/year |