**Company Brief**

|  |  |  |
| --- | --- | --- |
| **Year Founded** | : | 2012 |
| **Location** | : | Batang, Central Java, Indonesia |
| **Factory Space** | : | Plot size: 68,000 m2Built-up area: 28,200 m2 |
| **Industry** | : | Papermaking  |
| **Products** | : | 100% recycled brown kraft paper (100-200 GSM) of the following types:* Corrugating Medium
* Test Liner
 |
| **Production Capacity** | : | 115,000 MT/year |
| **Markets Served** | : | * Domestic
* International, including:
	+ China
	+ Southeast Asia
	+ South Asia
	+ Europe
	+ Middle East
	+ Africa
	+ ANZ
	+ Oceania
 |
| **Raw Material Source** | : | * Domestic
* International, including:
	+ Southeast Asia
	+ Europe
	+ Australia
	+ Africa
	+ Middle East
 |
| **Main Machines** | : | * European paper machine
* Machine width 4,500 mm
* 2 headboxes with fourdrinier table
* 51 dryers
* German-made pond sizer (Bellmer)
* Metso QCS and DCS
* Valmet rewinder twin drum
 |
| **Boilers** | : | 3 Boilers:* 1 x 20 tons
* 2 x 10 tons
 |
| **Waste Water Treatment** | : | * 5,000 m3 per day
* Designed to accommodate two paper machines
 |
| **Number of Employees** | : | 300 |
| **Electrical Power Supply** | : | PLN 8 Mva, backup generator 500 Kva |
| **Water Supply** | : | River and underground water source |
| **Additional Machines Procured but Not Installed** | : | * Disperger
* Refiners
 |
| **Average Revenue Growth** | : | 9.6%/year |